Step 1. Below output shows how to read the Serial Number from the DUT using the “AT+ECCRDSER“ command. Please refer to the AT command reference manual to know the details about the syntax of the AT command and the expected output.

A close up of numbers

Description automatically generated

**Note:** Serial number (Common Name) is prefixed with sn, so serial number becomes “sn0123C7E756AF138601”.